{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":16,"n_cols":8,"rows_kept":16,"flags":["formulas_cached_only"]}
["Erstellt von:","MHe"]
["Erstellt am:","2013-07-05"]
["GC:","V1.33-067"]
[]
["Programmstart und -ende mit den aufgeführten Einstellungen:"]
[]
[null,"Web-Server","DSFG DFÜ","Modbus TCP/IP","Fernbedienung","1. Ergebnis","Lösung","1. Ergebnis"]
[null,"BEIDE","BEIDE","BEIDE","BEIDE","Nothing to report for now","-","Nothing to report for now"]
[null,"BEIDE","BEIDE","BEIDE","LAN1","Nothing to report for now","-","Nothing to report for now"]
[null,"BEIDE","BEIDE","BEIDE","LAN2","Nothing to report for now","-","Nothing to report for now"]
[null,"BEIDE","BEIDE","LAN1","BEIDE","Nothing to report for now","-","Nothing to report for now"]
[null,"BEIDE","BEIDE","LAN2","BEIDE","closesocket() missing","~CModbusSlaveTCPIP(), closesocket()","Nothing to report for now"]
[null,"BEIDE","LAN1","BEIDE","BEIDE","Nothing to report for now","-","Nothing to report for now"]
[null,"BEIDE","LAN2","BEIDE","BEIDE","Nothing to report for now","-","Nothing to report for now"]
[null,"LAN1","BEIDE","BEIDE","BEIDE","Nothing to report for now","-","Nothing to report for now"]
[null,"LAN2","BEIDE","BEIDE","BEIDE","WSACleanup() missing","mg_start(), 3x WSACleanup()","Nothing to report for now"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}