{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":359,"n_cols":7,"rows_kept":359,"flags":["formulas_cached_only"]}
[1,"Fehler","Warnung",7001,"-","Konfig Datei falsch"]
[2,"Fehler","Warnung",7002,"-","Laden Signaturschlüssel","vorher 35"]
[3,"Fehler","Warnung",424,"-","AD-Wandler Bereich"]
[]
[]
[]
[]
[8,"Fehler","Rechnerfehler",407,"CAL|ANA","Neustart GC9300"]
[9,"Fehler","Rechnerfehler",407,"CAL|ANA","Neustart GC9300 (Bios)"]
[10,"Fehler","Warnung",7010,"-","T1 Leitungsbruch"]
[11,"Fehler","Warnung",7011,"-","T2 Leitungsbruch"]
[12,"Fehler","Warnung",7012,"-","Temp.-1 Alarmgrenzen"]
[13,"Fehler","Warnung",7013,"-","Temp.-2 Alarmgrenzen"]
[14,"Fehler","Warnung",621,"-","Stromausg.-1 Alarmgrenzen"]
[15,"Fehler","Warnung",622,"-","Stromausg.-2 Alarmgrenzen"]
[16,"Fehler","Warnung",623,"-","Stromausg.-3 Alarmgrenzen"]
[17,"Fehler","Warnung",624,"-","Stromausg.-4 Alarmgrenzen"]
[]
[]
[20,"Fehler","Rechnerfehler",7020,"CAL|ANA","ISO Bedingungen"]
[21,"Fehler","Rechnerfehler",7021,"CAL|ANA","GPA Bedingungen"]
[]
[]
[]
[25,"Fehler","Warnung",7025,"-","Nicht eichamtlich"]
[]
[]
[]
[]
[30,"Fehler","Rechnerfehler",7030,"CAL|ANA","Stickstoff Min/Max","Neu!"]
[31,"Fehler","Rechnerfehler",7031,"CAL|ANA","Methan Min/Max","Neu!"]
[32,"Fehler","Rechnerfehler",7032,"CAL|ANA","Kohlendioxid Min/Max","Neu!"]
[33,"Fehler","Rechnerfehler",7033,"CAL|ANA","Ethan Min/Max","Neu!"]
[34,"Fehler","Rechnerfehler",7034,"CAL|ANA","Propan Min/Max","Neu!"]
[35,"Fehler","Rechnerfehler",7035,"CAL|ANA","iso-Butan Min/Max","Neu!"]
[36,"Fehler","Rechnerfehler",7036,"CAL|ANA","n-Butan Min/Max","Neu!"]
[37,"Fehler","Rechnerfehler",7037,"CAL|ANA","neo-Pentan Min/Max","Neu!"]
[38,"Fehler","Rechnerfehler",7038,"CAL|ANA","iso-Pentan Min/Max","Neu!"]
[39,"Fehler","Rechnerfehler",7039,"CAL|ANA","n-Pentan Min/Max","Neu!"]
[40,"Fehler","Rechnerfehler",7040,"CAL|ANA","C6+ Min/Max","Neu!"]
[41,"Fehler","Rechnerfehler",7041,"CAL|ANA","n-Hexan Min/Max","Neu!"]
[42,"Fehler","Rechnerfehler",7042,"CAL|ANA","n-Heptan Min/Max","Neu!"]
[43,"Fehler","Rechnerfehler",7043,"CAL|ANA","n-Octan Min/Max","Neu!"]
[44,"Fehler","Rechnerfehler",7044,"CAL|ANA","n-Nonan Min/Max","Neu!"]
[45,"Fehler","Rechnerfehler",7045,"CAL|ANA","Sauerstoff Min/Max","Neu!"]
[46,"Fehler","Rechnerfehler",7046,"CAL|ANA","Helium Min/Max","Neu!"]
[47,"Fehler","Rechnerfehler",7047,"CAL|ANA","Wasserstoff Min/Max","Neu!"]
[48,"Fehler","Rechnerfehler",7048,"CAL|ANA","Argon Min/Max","Neu!"]
[49,"Fehler","Rechnerfehler",7049,"CAL|ANA","Reserve Min/Max","Neu!"]
[50,"Fehler","Rechnerfehler",7050,"CAL|ANA","Messwerk Timeout"]
[]
[52,"Fehler","Rechnerfehler",7052,"CAL|ANA","Messzeit max."]
[53,"Fehler","Rechnerfehler",7053,"CAL|ANA","Falsche Messwerk Nr."]
[]
[]
[]
[]
[]
[]
[60,"Fehler","Warnung",7060,"-","Wago AO1 Alarmgrenzen"]
[61,"Fehler","Warnung",7061,"-","Wago AO2 Alarmgrenzen"]
[62,"Fehler","Warnung",7062,"-","Wago AO3 Alarmgrenzen"]
[63,"Fehler","Warnung",7063,"-","Wago AO4 Alarmgrenzen"]
[64,"Fehler","Warnung",7064,"-","Wago AO5 Alarmgrenzen"]
[65,"Fehler","Warnung",7065,"-","Wago AO6 Alarmgrenzen"]
[66,"Fehler","Warnung",7066,"-","Wago AO7 Alarmgrenzen"]
[67,"Fehler","Warnung",7067,"-","Wago AO8 Alarmgrenzen"]
[68,"Fehler","Warnung",7068,"-","Wago AO9 Alarmgrenzen"]
[69,"Fehler","Warnung",7069,"-","Wago AO10 Alarmgrenzen"]
[70,"Fehler","Warnung",7070,"-","Wago AO11 Alarmgrenzen"]
[71,"Fehler","Warnung",7071,"-","Wago AO12 Alarmgrenzen"]
[72,"Fehler","Warnung",7072,"-","Wago AO13 Alarmgrenzen"]
[73,"Fehler","Warnung",7073,"-","Wago AO14 Alarmgrenzen"]
[74,"Fehler","Warnung",7074,"-","Wago AO15 Alarmgrenzen"]
[75,"Fehler","Warnung",7075,"-","Wago AO16 Alarmgrenzen"]
[]
[]
[]
[]
[80,"Fehler","Störung",7080,"ANA","Stickstoff §Min/Max","Neuer Text & umbenannt"]
[81,"Fehler","Störung",7081,"ANA","Methan §Min/Max","Neuer Text & umbenannt"]
[82,"Fehler","Störung",7082,"ANA","Kohlendioxid §Min/Max","Neuer Text & umbenannt"]
[83,"Fehler","Störung",7083,"ANA","Ethan §Min/Max","Neuer Text & umbenannt"]
[84,"Fehler","Störung",7084,"ANA","Propan §Min/Max","Neuer Text & umbenannt"]
[85,"Fehler","Störung",7085,"ANA","iso-Butan §Min/Max","Neuer Text & umbenannt"]
[86,"Fehler","Störung",7086,"ANA","n-Butan §Min/Max","Neuer Text & umbenannt"]
[87,"Fehler","Störung",7087,"ANA","neo-Pentan §Min/Max","Neuer Text & umbenannt"]
[88,"Fehler","Störung",7088,"ANA","iso-Pentan §Min/Max","Neuer Text & umbenannt"]
[89,"Fehler","Störung",7089,"ANA","n-Pentan §Min/Max","Neuer Text & umbenannt"]
[90,"Fehler","Störung",7090,"ANA","C6+ §Min/Max","Neuer Text & umbenannt"]
[91,"Fehler","Störung",7091,"ANA","n-Hexan §Min/Max","Neuer Text & umbenannt"]
[92,"Fehler","Störung",7092,"ANA","n-Heptan §Min/Max","Neuer Text & umbenannt"]
[93,"Fehler","Störung",7093,"ANA","n-Octan §Min/Max","Neuer Text & umbenannt"]
[94,"Fehler","Störung",7094,"ANA","n-Nonan §Min/Max","Neuer Text & umbenannt"]
[95,"Fehler","Störung",7095,"ANA","Sauerstoff §Min/Max","Neuer Text & umbenannt"]
[96,"Fehler","Störung",7096,"ANA","Helium §Min/Max","Neuer Text & umbenannt"]
[97,"Fehler","Störung",7097,"ANA","Wasserstoff §Min/Max","Neuer Text & umbenannt"]
[98,"Fehler","Störung",7098,"ANA","Argon §Min/Max","Neuer Text & umbenannt"]
[99,"Fehler","Störung",7099,"ANA","Reserve §Min/Max","Neuer Text & umbenannt"]
[100,"Fehler","Störung",609,"CAL","Kal: Retentionszeit"]
[101,"Fehler","Störung",610,"CAL","Response Faktor"]
[102,"Fehler","Störung",608,"CAL","Kal: unnorm. Sum."]
[103,"Fehler","Störung",7103,"CAL","Kal: Gesamtfläche"]
[104,"Fehler","Störung",7104,"CAL","Kal: Konzentration"]
[105,"Fehler","Störung",7105,"CAL","Kal: HO Grenzwert"]
[106,"Fehler","Störung",7106,"CAL","Kal: Rhon Grenzwert"]
[107,"Fehler","Störung",7107,"CAL","Kal: CO2 Grenzwert"]
{"$rows_empty":12}
[120,"Fehler","Störung",7120,"ANA","Ana: Retentionszeit"]
[121,"Fehler","Störung",7121,"ANA","Ana: unnorm. Sum."]
[122,"Fehler","Störung",7122,"ANA","Ana: Konzentration"]
[123,"Fehler","Störung",7123,"ANA","Ana: Ho Min/Max"]
[124,"Fehler","Störung",7124,"ANA","Ana: Wo Min/Max"]
[125,"Fehler","Störung",7125,"ANA","Ana: Mz Min/Max"]
[126,"Fehler","Störung",7126,"ANA","Ana: DV Min/Max"]
[127,"Fehler","Störung",7127,"ANA","Ana: Rho,n Min/Max"]
[]
[]
[130,"Fehler","Störung",7130,"CAL|ANA","Druck des Meßgases"]
[131,"Fehler","Störung",7131,"CAL|ANA","Trägergasdruck -I"]
[132,"Fehler","Störung",7132,"CAL|ANA","Trägergasdruck -II"]
{"$rows_empty":16}
[149,"Fehler","Störung",7149,"CAL|ANA","Methode nicht gefunden"]
[150,"Warnung","Warnung",7150,"-","Kal: Konzentration"]
[151,"Warnung","Warnung",7151,"-","Ana: Konzentration"]
[152,"Warnung","Warnung",7152,"-","Temp.-1 Warngrenzen"]
[153,"Warnung","Warnung",7153,"-","Temp.-2 Warngrenzen"]
[154,"Warnung","Warnung",7154,"-","Stromausg.-1 Warngrenzen"]
[155,"Warnung","Warnung",7155,"-","Stromausg.-2 Warngrenzen"]
[156,"Warnung","Warnung",7156,"-","Stromausg.-3 Warngrenzen"]
[157,"Warnung","Warnung",7157,"-","Stromausg.-4 Warngrenzen"]
[158,"Warnung","Warnung",7158,"-","#DiWarnText_0"]
[159,"Warnung","Warnung",7159,"-","#DiWarnText_1"]
[160,"Warnung","Warnung",7160,"-","#DiWarnText_2"]
[161,"Warnung","Warnung",7161,"-","#DiWarnText_3"]
[162,"Warnung","Warnung",7162,"-","#DiWarnText_4"]
[163,"Warnung","Warnung",7163,"-","#DiWarnText_5"]
[164,"Warnung","Warnung",7164,"-","#DiWarnText_6"]
[165,"Warnung","Warnung",7165,"-","#DiWarnText_7"]
[166,"Warnung","Warnung",7166,"-","#DiWarnText_8"]
[167,"Warnung","Warnung",7167,"-","#DiWarnText_9"]
[168,"Warnung","Warnung",7168,"-","#DiWarnText_10"]
[169,"Warnung","Warnung",7169,"-","#DiWarnText_11"]
[170,"Warnung","Warnung",7170,"-","#DiWarnText_12"]
[171,"Warnung","Warnung",7171,"-","#DiWarnText_13"]
[172,"Warnung","Warnung",7172,"-","#DiWarnText_14"]
[173,"Warnung","Warnung",7173,"-","#DiWarnText_15"]
[174,"Warnung","Warnung",7174,"-","#DiWarnText_16"]
[175,"Warnung","Warnung",7175,"-","#DiWarnText_17"]
[176,"Warnung","Warnung",7176,"-","#DiWarnText_18"]
[177,"Warnung","Warnung",7177,"-","#DiWarnText_19"]
[]
[179,"Warnung","-",0,"-","Grenzwert H2S-Summe"]
[180,"Warnung","Warnung",7180,"-","Stickstoff §Min/Max","Neuer Text & umbenannt"]
[181,"Warnung","Warnung",7181,"-","Methan §Min/Max","Neuer Text & umbenannt"]
[182,"Warnung","Warnung",7182,"-","Kohlendioxid §Min/Max","Neuer Text & umbenannt"]
[183,"Warnung","Warnung",7183,"-","Ethan §Min/Max","Neuer Text & umbenannt"]
[184,"Warnung","Warnung",7184,"-","Propan §Min/Max","Neuer Text & umbenannt"]
[185,"Warnung","Warnung",7185,"-","iso-Butan §Min/Max","Neuer Text & umbenannt"]
[186,"Warnung","Warnung",7186,"-","n-Butan §Min/Max","Neuer Text & umbenannt"]
[187,"Warnung","Warnung",7187,"-","neo-Pentan §Min/Max","Neuer Text & umbenannt"]
[188,"Warnung","Warnung",7188,"-","iso-Pentan §Min/Max","Neuer Text & umbenannt"]
[189,"Warnung","Warnung",7189,"-","n-Pentan §Min/Max","Neuer Text & umbenannt"]
[190,"Warnung","Warnung",7190,"-","C6+ §Min/Max","Neuer Text & umbenannt"]
[191,"Warnung","Warnung",7191,"-","n-Hexan §Min/Max","Neuer Text & umbenannt"]
[192,"Warnung","Warnung",7192,"-","n-Heptan §Min/Max","Neuer Text & umbenannt"]
[193,"Warnung","Warnung",7193,"-","n-Octan §Min/Max","Neuer Text & umbenannt"]
[194,"Warnung","Warnung",7194,"-","n-Nonan §Min/Max","Neuer Text & umbenannt"]
[195,"Warnung","Warnung",7195,"-","Sauerstoff §Min/Max","Neuer Text & umbenannt"]
[196,"Warnung","Warnung",7196,"-","Helium §Min/Max","Neuer Text & umbenannt"]
[197,"Warnung","Warnung",7197,"-","Wasserstoff §Min/Max","Neuer Text & umbenannt"]
[198,"Warnung","Warnung",7198,"-","Argon §Min/Max","Neuer Text & umbenannt"]
[199,"Warnung","Warnung",7199,"-","Reserve §Min/Max","Neuer Text & umbenannt"]
[200,"Warnung","Warnung",7200,"-","Druck des Meßgases"]
[201,"Warnung","Warnung",7201,"-","Messwerk Timeout"]
[]
[203,"Warnung","Warnung",7203,"-","Zu viele Peaks"]
[204,"Warnung","Warnung",7204,"-","Wago AO1 Warngrenzen"]
[205,"Warnung","Warnung",7205,"-","Wago AO2 Warngrenzen"]
[206,"Warnung","Warnung",7206,"-","Wago AO3 Warngrenzen"]
[207,"Warnung","Warnung",7207,"-","Wago AO4 Warngrenzen"]
[208,"Warnung","Warnung",7208,"-","Wago AO5 Warngrenzen"]
[209,"Warnung","Warnung",7209,"-","Wago AO6 Warngrenzen"]
[210,"Warnung","Warnung",7210,"-","Wago AO7 Warngrenzen"]
[211,"Warnung","Warnung",7211,"-","Wago AO8 Warngrenzen"]
[212,"Warnung","Warnung",7212,"-","Wago AO9 Warngrenzen"]
[213,"Warnung","Warnung",7213,"-","Wago AO10 Warngrenzen"]
[214,"Warnung","Warnung",7214,"-","Wago AO11 Warngrenzen"]
[215,"Warnung","Warnung",7215,"-","Wago AO12 Warngrenzen"]
[216,"Warnung","Warnung",7216,"-","Wago AO13 Warngrenzen"]
[217,"Warnung","Warnung",7217,"-","Wago AO14 Warngrenzen"]
[218,"Warnung","Warnung",7218,"-","Wago AO15 Warngrenzen"]
[219,"Warnung","Warnung",7219,"-","Wago AO16 Warngrenzen"]
[220,"Hinweis","Hinweis",7220,"-","MZ Eingabewerte"]
[221,"Hinweis","Hinweis",7221,"-","Ventile fixiert"]
[222,"Hinweis","-",0,"-","Testbetrieb"]
[223,"Hinweis","Hinweis",7223,"-","Kal: Vorgabewerte"]
[224,"Hinweis","Hinweis",7224,"-","Drucker nicht bereit"]
[225,"Hinweis","Hinweis",7225,"-","EVars CRC"]
[226,"Hinweis","Hinweis",7226,"-","BVars CRC"]
[227,"Hinweis","Hinweis",7227,"-","Testmodus Dig. Ausgänge"]
[228,"Hinweis","Hinweis",7228,"-","Abgleichwerte Ferro(CRC)"]
[229,"Hinweis","Hinweis",7229,"-","Abgleichwerte Ferro(Ver)"]
[230,"Hinweis","Hinweis",800,"-","Eichschloss"]
[231,"Hinweis","Hinweis",801,"-","Codewort"]
[232,"Hinweis","Hinweis",810,"-","Alte Uhrzeit"]
[233,"Hinweis","Hinweis",811,"-","Neue Uhrzeit"]
[234,"Hinweis","Hinweis",802,"-","Revision"]
[235,"Hinweis","Hinweis",7235,"-","Schreibe Simufile"]
[236,"Hinweis","Hinweis",7236,"-","EichamtlicheIBN!"]
[237,"Hinweis","Hinweis",7237,"-","GBM ext. Prüfgas"]
[]
[]
[240,"Hinweis","Hinweis",7240,"-","Multilevel Import ok"]
[241,"Hinweis","Hinweis",7241,"-","Multilevel Import nok"]
[242,"Hinweis","Hinweis",7242,"-","Messwerk Initializing"]
[243,"Hinweis","Hinweis",7243,"-","Messwerk Flushing"]
[]
[]
[]
[247,"Hinweis","Hinweis",760,"-","Messwerk kalibriert"]
[]
[]
[250,"Hinweis","Hinweis",7250,"-","Chromatogramm (FTP)"]
[251,"Hinweis","Hinweis",7251,"-","FlushChromatogramm (FTP)"]
[252,"Hinweis","Hinweis",7252,"-","Schreiben Chrom"]
[253,"Hinweis","Hinweis",7253,"-","Schreiben FlushChrom"]
[]
[]
[]
[]
[]
[]
[260,"Hinweis","Hinweis",7260,"-","Ausheizen"]
[261,"Hinweis","Hinweis",7261,"-","Abkühlen"]
[262,"Hinweis","Hinweis",7262,"-","Equilibrieren"]
[263,"Hinweis","Hinweis",7263,"-","MW Setzen Messmeth. NOK"]
[264,"Hinweis","Hinweis",7264,"-","MW Setzen Messmeth. OK"]
[]
[]
[]
[]
[]
[270,"Hinweis","Hinweis",7270,"-","Parameterlog deaktiviert"]
[271,"Hinweis","-",0,"-","Uhrzeit alt"]
[272,"Hinweis","-",0,"-","Uhrzeit neu"]
{"$rows_empty":27}
[300,"Warnung","Warnung",7300,"-","Stromeing-1 Warngrenzen"]
[301,"Warnung","Warnung",7301,"-","Stromeing-2 Warngrenzen"]
[302,"Warnung","Warnung",7302,"-","Stromeing-3 Warngrenzen"]
[303,"Warnung","Warnung",7303,"-","Stromeing-4 Warngrenzen"]
[304,"Warnung","Warnung",7304,"-","Stromeing-5 Warngrenzen"]
[305,"Warnung","Warnung",7305,"-","Stromeing-6 Warngrenzen"]
[306,"Warnung","Warnung",7306,"-","Stromeing-7 Warngrenzen"]
[307,"Warnung","Warnung",7307,"-","Stromeing-8 Warngrenzen"]
[308,"Warnung","Warnung",7308,"-","Abbruch Ausheizen -> Messmeth. setzen"]
[]
[310,"Warnung","Warnung",7310,"-","Wago AI1 Warngrenzen"]
[311,"Warnung","Warnung",7311,"-","Wago AI2 Warngrenzen"]
[312,"Warnung","Warnung",7312,"-","Wago AI3 Warngrenzen"]
[313,"Warnung","Warnung",7313,"-","Wago AI4 Warngrenzen"]
[314,"Warnung","Warnung",7314,"-","Wago AI5 Warngrenzen"]
[315,"Warnung","Warnung",7315,"-","Wago AI6 Warngrenzen"]
[316,"Warnung","Warnung",7316,"-","Wago AI7 Warngrenzen"]
[317,"Warnung","Warnung",7317,"-","Wago AI8 Warngrenzen"]
[318,"Warnung","Warnung",7318,"-","Wago AI9 Warngrenzen"]
[319,"Warnung","Warnung",7319,"-","Wago AI10 Warngrenzen"]
[320,"Warnung","Warnung",7320,"-","Wago AI11 Warngrenzen"]
[321,"Warnung","Warnung",7321,"-","Wago AI12 Warngrenzen"]
[322,"Warnung","Warnung",7322,"-","Wago AI13 Warngrenzen"]
[323,"Warnung","Warnung",7323,"-","Wago AI14 Warngrenzen"]
[324,"Warnung","Warnung",7324,"-","Wago AI15 Warngrenzen"]
[325,"Warnung","Warnung",7325,"-","Wago AI16 Warngrenzen"]
[]
[]
[]
[]
[330,"Warnung","Warnung",7330,"-","Multistream Parameter"]
[331,"Warnung","Warnung",7331,"-","Lesen Dil-Schalter"]
[332,"Warnung","Warnung",7332,"-","Explorer läuft!"]
[333,"Warnung","Warnung",7333,"-","Speichern Displaykal."]
[334,"Warnung","Warnung",7334,"-","Software-Neustart MW"]
[335,"Warnung","Warnung",7350,"-","CP-Daten"]
[]
[]
[]
[]
[340,"Warnung","Warnung",7340,"-","Stickstoff Min/Max","Neu!"]
[341,"Warnung","Warnung",7341,"-","Methan Min/Max","Neu!"]
[342,"Warnung","Warnung",7342,"-","Kohlendioxid Min/Max","Neu!"]
[343,"Warnung","Warnung",7343,"-","Ethan Min/Max","Neu!"]
[344,"Warnung","Warnung",7344,"-","Propan Min/Max","Neu!"]
[345,"Warnung","Warnung",7345,"-","iso-Butan Min/Max","Neu!"]
[346,"Warnung","Warnung",7346,"-","n-Butan Min/Max","Neu!"]
[347,"Warnung","Warnung",7347,"-","neo-Pentan Min/Max","Neu!"]
[348,"Warnung","Warnung",7348,"-","iso-Pentan Min/Max","Neu!"]
[349,"Warnung","Warnung",7349,"-","n-Pentan Min/Max","Neu!"]
[350,"Warnung","Warnung",7350,"-","C6+ Min/Max","Neu!"]
[351,"Warnung","Warnung",7351,"-","n-Hexan Min/Max","Neu!"]
[352,"Warnung","Warnung",7352,"-","n-Heptan Min/Max","Neu!"]
[353,"Warnung","Warnung",7353,"-","n-Octan Min/Max","Neu!"]
[354,"Warnung","Warnung",7354,"-","n-Nonan Min/Max","Neu!"]
[355,"Warnung","Warnung",7355,"-","Sauerstoff Min/Max","Neu!"]
[356,"Warnung","Warnung",7356,"-","Helium Min/Max","Neu!"]
[357,"Warnung","Warnung",7357,"-","Wasserstoff Min/Max","Neu!"]
[358,"Warnung","Warnung",7358,"-","Argon Min/Max","Neu!"]
[359,"Warnung","Warnung",7359,"-","Reserve Min/Max","Neu!"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}