{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["CompatibleMode_Klassen"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"CompatibleMode_Klassen","index":0,"n_rows":44,"n_cols":10,"rows_kept":44,"merged":[[0,0,0,3],[3,0,3,1],[3,2,3,3],[3,5,3,6]],"flags":["formulas_cached_only"]}
["CompatibleMode Klassen"]
[]
[]
["CGcCM : CGc",null,"CCP4002Prot",null,null,"CGc",null,null,"CMyTimer"]
["public:",null,"public:",null,null,"public:",null,null,"public:"]
[null,"CGcCM()",null,"CCP4002Prot()",null,null,"CGc()",null,null,"CMyTimer()"]
[null,"~CGcCM()",null,"~CCP4002Prot()",null,null,"~CGc()",null,null,"CMyTimer(…)"]
[null,"StartGcCM()",null,"StartCP4002ProtOnCan()",null,null,"WriteTimeToVarian()",null,null,"~CMyTimer()"]
[null,"StopGcCM()",null,"StopCP4002Prot()",null,null,"StartGc()",null,null,"StartTimer()"]
[{"$nulls":3},"ModeChanged()",null,null,"StopGc()",null,null,"StopTimer()"]
[{"$nulls":3},"ParamsChanged()",null,null,"SetSkip()",null,null,"ResetExpCounter()"]
[{"$nulls":3},"Transmit()",null,null,"IsCalibStart()",null,null,"DoesTimerExist()"]
[{"$nulls":3},"RecvFromCAN()",null,null,"SetMSInfoText()",null,null,"Get_NumberOfExpiry()"]
[{"$nulls":3},"SetCpStatusString()",null,null,"Autorun()",null,null,"Get_Akt_Secs()"]
[{"$nulls":6},"DoMessungFertig()",null,null,"Get_RunState()"]
[{"$nulls":6},"SetNextStreamPosAndNextCalcJob()"]
[]
["private:",null,"private:",null,null,"private:",null,null,"private:"]
[null,"_GcCMThreadFunc()",null,"Init()",null,null,"GcThreadFunc()",null,null,"_ThreadFunc()"]
[null,"GcCMThreadFunc()",null,"CleanUp()",null,null,"DoGc()",null,null,"ThreadFunc()"]
[null,"_GcCMThreadStatemachine()",null,"Trans()",null,null,"DoStep1()"]
[null,"GcCMThreadStatemachine()",null,"Recv()",null,null,"Simulation()"]
[null,"ReadMethod()",null,"ProcessRecvData()",null,null,"FillStepwerte()"]
[null,"CopyDataForCalc()",{"$nulls":4},"LogFile()"]
[null,"CopyDataForChrom()",{"$nulls":4},"WritePeakFile()"]
[null,"DeleteDataForChrom()",{"$nulls":4},"CopyParaFiles()"]
[null,"CopyDataForPeak()",{"$nulls":4},"CreateInfoFile()"]
[null,"DeleteDataForPeak()",{"$nulls":4},"GetFTPFile()"]
[null,"CopyDataForStatus()",{"$nulls":4},"ReadCP4900ChannelStatus()"]
[{"$nulls":6},"ShowSWStatus()"]
[{"$nulls":6},"CheckDSfGBitleisten()"]
[{"$nulls":6},"WriteCP4002ChromFile()"]
[{"$nulls":6},"WriteCP4002PeakFile()"]
[]
[]
[{"$nulls":5},"protected:"]
[{"$nulls":6},"InitFunc()"]
[{"$nulls":6},"ChangeStream()"]
[{"$nulls":6},"CarrierGas()"]
[{"$nulls":6},"SampleGas()"]
[{"$nulls":6},"CheckSpecialInput()"]
[{"$nulls":6},"CheckSumH2S()"]
[{"$nulls":6},"CurrentOutputs()"]
[{"$nulls":6},"CheckInputs()"]