{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Aufbau Chromfile","Aufbau Peakfile"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Aufbau Chromfile","index":0,"n_rows":11,"n_cols":3,"rows_kept":11,"merged":[[0,0,0,1]],"flags":["formulas_cached_only"]}
["Aufbau des Chromfiles"]
[]
["Datengröße","Bezeichnung","Erklärung"]
["int32","fileType","Fixer Wert: 0x7FFF0008"]
["int32","fileVersion","Fixer Wert: 0x1"]
["unsigned char [8]","date","Zeitstempel letztes Analysenende"]
["char [256]","info","-"]
["int32 [4]","numDataPoints [4]","Anzahl Datenpunkte pro Säule"]
["int32 [4]","freq [4]","Frequenz pro Säule"]
["char [128]","reserved","-"]
["int32 [4][numDataPoints[4]]","dataPoints[4][numDataPoints[4]]","Datenpunkte pro Säule"]

{"sheet":"Aufbau Peakfile","index":1,"n_rows":16,"n_cols":4,"rows_kept":16,"merged":[[0,0,0,2]],"flags":["formulas_cached_only"]}
["Aufbau des Peakfiles"]
[]
["Datengröße","Bezeichnung","Erklärung"]
["wchar_t [20]","header","Fixer Wert: \"RMG-Peak-File\""]
["float","version","Fixer Wert: 0x4"]
["int32","channels","Anzahl der Säulen"]
["int32 [3]","anzPeaks","Anzahl der Peaks pro Säule"]
["unsigned char [20]","reserved","-"]
["-","PEAKS","Peakdaten"]
[]
[null,"PEAKS"]
[null,"Datengröße","Bezeichnung","Erklärung"]
[null,"float [channels][anzPeaks[x]]","startTime","Starttime pro Peak pro Säule"]
[null,"float [channels][anzPeaks[x]]","stopTime","Stoptime pro Peak pro Säule"]
[null,"float [channels][anzPeaks[x]]","retentionTime","RT pro Peak pro Säule"]
[null,"wchar_t [channels][anzPeaks[x]]","name","Peakname pro Peak pro Säule"]